Use a 4mm compression bit for cutting.
There will be gaps that the lines don’t line up but this is designed that way . The gap is 4mm which is the size bit needed
Hardware used..
https://www.ebay.co.uk/itm/153630547817
https://www.ebay.co.uk/itm/166637041908?var=466294536250
https://www.ebay.co.uk/itm/376017835458?var=644822347909
https://www.ebay.co.uk/itm/141382827424?var=440525292018 500mm or 600mm runners. Depending on the size of the drawer
https://www.ironmongerydirect.co.uk/product/self-drive-dowel-cam-centrepin-length-34mm-black-pack-of-50-786691?mm_rf=mm_974b13682665ef5c7238
https://www.ironmongerydirect.co.uk/product/rimless-cam-connector-15mm-min-panel-thickness-nickel-plated-pack-of-50-325445?mm_rf=mm_974b13682665ef5c7238

If your doing cushions I can give you a guy I used to use for foam. Fabric I used to use
https://www.ebay.co.uk/itm/184441792665?var=692143901614


Each dxf files have 3-4 sheets already on there in each of its own box. Please select everything inc the outer box of each sheet and put in a new 1220x2440 size project.


🛠️ Camper Conversion Build Guide
🪑 Step 1: Build the Rear Seat Base (Wheel Arch Section)
The rear seat base is the first section to assemble. This includes the main panel with the wheel arch cut-outs, The rear panel and the seating panels x 4.
🔧 Assembly Instructions
· Take the main back panel with the wheel arch cut-outs and place it with the 15mm holes facing down. 
· Attach the two smaller side panels: 
· Position them flush against the curved wheel arch edges 
· Ensure the 15mm connection holes are facing outward (visible from the outside) 
· Secure each side panel using: 
· 30mm x 3.5 screws 
· 3 screws per side: 
· 2 near the front (around the cam holes) 
· 1 near the rear curve 
🔩 Top Panel Installation
· Position the top panels above the front and back panels. Make sure back panel the door opens the opposite way to the wheel arch panel. So back panel door opens out of the van, inner panel door opens inside the van.
🔗 2 outer Panel Connections
Use:
· 34mm cam dowels (pins) 
· Rimless cam connectors 
Steps:
· Insert cam dowels into pre-drilled holes 
· Place cam connectors into the 15mm holes 
· Ensure arrows face the correct direction 
· Tighten clockwise to lock panels together 
Place to 2 lift up panels in place and secure to the outers using 75mm brackets. 2 each side with 15mm screws
💡 Pro Tip:
Ensure all connection holes face inward under the seat before fixing

🧱 Step 2: Assemble the Driver Side Frame
🔧 Assembly Instructions
· Take the driver side front panel. 
· Insert: 
· 4 x cam dowels into the pre-drilled holes 
· Insert the panel into the side panel already fixed to the rear section. 
🧱 Add End Panel
· Attach the end panel to the front panel: 
· Align cam fittings 
· Insert cam connectors into the 15mm holes 
· Tighten clockwise to lock everything together 
🪑 Fit Top Panel
· Screw in 6 cam dowels to the underside
· Place the top panel onto the structure 
· Secure by locking all cam connectors 
· Ensure panels are square and tightly fitted 
💡 Pro Tip:
Check alignment before fully tightening to avoid issues later in the build.

🗄️ Step 3: Drawer System & Seat Mechanism
🔧 Install Drawer Runners
· On the back front panel of the passenger panel: 
· Position drawer runner: 
· 18mm up from the bottom 
· 18mm back from the drawer-side edge 
🧱 Fit Panels Together
· Install: 
· Front panel
· End panel 
· Back panel 

· On the long 67mm panel: 
· Attach matching runner: 
· 18mm up 
· Flush with the end 
· Secure the long inner panel using: 
· L brackets to front panel making sure its flush with the side of the end panel and drawer mech can be extended properly. 
· Screws 
· Ensure square alignment before tightening fully 
🗄️ Install Drawer
· Assemble the drawer unit 
· Position in the opening: 
· Raise 10mm off the ground using spacers 
· Extend runners until flush with the front 
· Screw runners into place 
· Measure the opening and secure the back L brackets so that thw distance between front panel and the runner panel is the same. Usually about 31cm.
🪑 Fit Top Panels
· Install the first top panel (with holes) with pin dowels and lock those in place with the cam locks
· Place the second panel above it: 
· This will fold over to form the bed 
🔵 Rounded Front Panels
Attach 40mm rounded panels to the front of passenger and drivers side panels:
· Driver side: 36mm down from top 
· Passenger side: 18mm down from top 
Fix using:
· Glue 
· Screws 
🛏️ Final Seat Panel
· Place remaining seat panel in the middle and flush with the drawer side: 
· Flush on drawer side (2mm smaller) 
· Centered in bed position (should be a 4mm gap each side)
· Secure using: 
· 75mm hinges x 2
🦵 Support Leg (Recommended)
· Create leg from 2 passenger seat offcuts: 
· Glue and screw together flush 
· Cut to correct height 
· Install using: 
· 150mm T hinge 
· 15mm screws into bed panel 
· 30mm screws into leg 
💡 Acts as a folding support when bed is extended.

🍳 Step 4: Assemble the Kitchen Unit
🔧 Build the Kitchen Frame
· Start with the front panel: 
· Insert all cam dowels 
· Attach side panels: 
· Ensure shelf pin holes face inward 
📏 Shelf Pin Setup (If Required)
· Drill holes where needed: 
· 3 inches from front and back 
· Mid-height of panel 
· Use: 
· 4.5–4.8mm drill bit 
· 7mm depth 
· Insert shelf pins before full assembly 
🧊 Fridge Unit Setup (If Applicable)
Drill front panel fixing holes:
· Measure 391mm from back edge on the larger panels with the 15mm holes facing down. Make sure you position it so top is away from you and measure right to left
· Drill: 
· 2 inches from bottom 
· 2 inches from top 
· 1 centered 
🧱 Complete Cabinet
· Insert cam connectors into 15mm holes 
· Tighten clockwise 
· Attach top panel using cam locks 
· Ensure structure is square 
🪑 Table Installation (Optional)
· Place table (best side down) 
· Centre mounting bracket 
· Fix using: 
· 6 x 20mm x5 screws 
🚐 Fixing Into Van
Secure using:
· 40mm L brackets: 
· 2 rear outer panel 
· 2 passenger side (middle) 
· 1 near drawer area 
· Kitchen base fixing: 
· 30mm screws into driver-side end panel from inside kitchen cabinet
· 2 brackets on opposite side either end fridge panel or inside left door
· 15mm screws into wooden floor (if applicable) 
💡 Always dry-fit before final installation.

💡 Final Tips & Notes
🛠️ Build Before Installing
· Assemble the unit fully outside the van first 
· This ensures: 
· Proper alignment 
· Easier adjustments 
· Smooth installation 
🔄 Disassembly
· Each side can be removed as a single piece by: 
· Unscrewing the 3 screws on the wheel arch sections 
· The rear section must be fully dismantled 
💡 Keep components grouped (rear, driver side, passenger side, kitchen) for easier handling.

Final Note
Not all van makes are the same internally. Some vans might need a little scribing if ply lining is slightly different.
You might do like a T5 and no scribing require and another T5 can come in and its slightly narrower.
